|  |  |
| --- | --- |
| TNC Testing Form (REV1) | |
| Leaf on the Tree | DAC |
| Device Under Test (Testing Tree Number): | 2.3.2 |
| Date: | 11/1/20 |
| Person(s) Conducting Experiment: | Kobe Keopraseuth, Kaleb Leon, David Cain |
| Signature: |  |
| Experiment Purpose: | Test the entire DAC subsystem with an actual AX.25 packet actually used in our project. |
| Experiment Procedure: | Feed a known accurate AX.25 packet then use code to covert that into an analog output signal. |
| Equipment Settings / Software Settings (w Revision): | Current code base for DAC Sinewave. |
| Testing Diagram / Picture: |  |
| Data Points: |  |
| Pass / Fail: | Pass |
| Interpreted Notes: | Meets the accuracy we required of the output analog signal. |
| Recommendations for Modifications: | N/A |